{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"flags":["formulas_cached_only"]}
[{"$nulls":4},"PERFORMANCE OF \"THE DI PIETRO  MOTOR\""]
[]
[]
["The following testings were conducted on Saturday the 6th of June 2009"]
["The engine is 6 chambers total 265cc"]
["The results are:"]
[]
[]
[]
["Potenza","Coppia","Giri","Pressure entrata","Consumo a pressione ambiente","Consumo per cavallo di forza"]
["OUTPUT POWER","TORQUE","SPEED","INLET PRESSURE","CONSUMPTION AT TOTAL OUTPUT","CONSUMPTION PER HORSEPOWER","ENGINE WEIGHT","efficiency"]
["(hp)","(Nm)","(rpm)","(psi)","(S/L/min)","(S/L/min)","(kg)"]
[{"$nulls":5}," "]
[3.725,24,1102,141,1250,335,13]
[3.821,21.94,1240,138,1250,327,13]
[3.827,17.95,1517,135,1300,339,13]
[3.803,20.68,1309,136,1200,315,13]
[3.341,26,920,139,1000,299,13]
[3.839,21,1318,134,1200,312,13]
[3.823,21.25,1281,136,1200,313,13]
[0.4026,4.669,613.9,25.11,347,null,13,{"v":0.945,"d":"94.50%"},null,"Tested just resently"]
["The following testings were conducted on the 27th October 2009"]
["The engine is the new generation 9 chambers total 399cc"]
["The results are:"]
[]
[]
[]
[]
[]
["OUTPUT POWER","TORQUE","SPEED","INLET PRESSURE","CONSUMPTION AT TOTAL OUTPUT","CONSUMPTION PER HORSEPOWER","ENGINE WEIGHT"]
["(hp)","(Nm)","(rpm)","(psi)","(S/L/min)","(S/L/min)","(kg)"]
[]
[3.918,34.42,810,159,1150,293,9.5]
[4.949,28.32,1244,158,1450,292,9.5]
[5.422,29.47,1310,166,1400,258,9.5]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}